# Acronyms

Weatherization Assistance Program Standardized Training Curricula

|  |  |
| --- | --- |
| ABS | Acryonitrile Butadiene Styrene |
| ACCA | Air Conditioning Contractors of America |
| ACH | Air Changes per Hour |
| AEE | Association of Energy Engineers |
| AGA | American Gas Association |
| AHAM | Association of Home Appliance Manufacturers |
| AHU | Air-Handling Unit |
| ANSI | American National Standards Institute |
| ARRA | American Recovery and Reinvestment Act |
| ASC | Accredited Standards Committee |
| ASHRAE | American Society of Heating, Refrigerating and Air Conditioning Engineers |
| BMS | Building Management System |
| BPI | Building Performance Institute |
| BTL | Building Tightness Limit |
| BTU | British Thermal Units |
| CAA | Community Action Agency |
| CAP | Community Action Program, or Community Action Agency |
| CAZ | Combustion Appliance Zone |
| CFH | Cubic Feet per Hour |
| CFL | Compact Fluorescent Lamp |
| CFM | Cubic Feet per Minute |
| CO | Carbon Monoxide |
| CO2 | Carbon Dioxide |
| CRF | Can’t Reach Fifty |
| CRI | Color Rendering Index |
| DHW | Domestic Hot Water |
| DHWT | Domestic Hot Water Tank |
| DOE | Department of Energy |
| DOE PO | DOE Project Officer |
| DTL | Depressurization Tightness Limit |
| EAI | Energy Audit Institute |

|  |  |
| --- | --- |
| EA-QUIP | Energy Audit Using the Queens Information Package |
| EDL | Equivalent Duct Length |
| EIA | Energy Information Administration |
| ELA | Equivalent Leakage Area |
| EPA | Environmental Protection Agency |
| FIFO | First-in, First-out System |
| GFCI | Ground Fault Circuit Interrupter |
| GVW | Gross Vehicle Weight |
| H&S | Health and Safety |
| HDD | Heating Degree Days |
| HERS | Home Energy Rating System |
| HRV | Heat Recovery Ventilation |
| HUD | Housing and Urban Development |
| HVAC | Heating, Ventilating, and Air Conditioning |
| HVI | Home Ventilating Institute |
| IAPMO | International Association of Plumbing and Mechanical Officials |
| IAQ | Indoor Air Quality |
| ICC | International Codes Council |
| IC | Insulating Contact |
| IFGC | International Fuel Gas Code |
| IR | Infrared |
| IRC | International Residential Code |
| IWC | Inches of water column |
| LBNL | Lawrence Berkeley National Laboratory (also written LBL) |
| LEED | Leadership in Energy and Environmental Design |
| LIHEAP | Low Income Home Energy Assistance Program |
| LPG | Liquefied Petroleum Gas |
| LSW | Lead Safe Weatherization |
| MF | Multifamily |
| MHEA | Manufactured Home Energy Audit |
| MRT | Mean Radiant Temperature |
| MSDS | Material Safety Data Sheet |
| MVG | Minimum Ventilation Guideline |
| MVR | Minimum Ventilation Requirement |
| NEAT | National Energy Audit Tool |
| NEC | National Electrical Code |

|  |  |
| --- | --- |
| NFA | Net Free Area (in reference to ventilation standards) |
| NFPA | National Fire Protection Association |
| NFRC | National Fenestration Rating Council |
| NIOSH | National Institute for Occupational Safety and Health |
| o.c. | On Center |
| ORNL | Oak Ridge National Laboratory |
| OSHA | Occupational Safety and Health Administration |
| Pa | Pascals |
| PHA | Public Housing Authority or Agency |
| PMC | Project Management Center |
| PPE | Personal Protection Equipment |
| PPM | Parts Per Million |
| PSI | Pounds Per Square Inch |
| PV | Present Value |
| QC | Quality Control |
| RH | Relative Humidity |
| SC | Shading Coefficient |
| SF | Single Family |
| SHGC | Solar Heat Gain Coefficient |
| SIR | Savings-to-Investment Ratio |
| SO2 | Sulfur Dioxide |
| T&TA | Training and Technical Assistance |
| TREAT | Targeted Retrofit Energy Analysis Tool |
| WAP | Weatherization Assistance Program |
| WPN | Weatherization Program Notice |
| WRT | With Reference To |
| ZPD | Zone Pressure Diagnostics |